;****************************************************************************************
;
;   mtkwecx.inf
;   MediaTek Wireless LAN card installation script
;
;   MediaTek Inc. (C)2022. All rights reserved.
;
;****************************************************************************************

[Version]
Signature       = "$Windows NT$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %MediaTek%
CatalogFile     = mtkwecx.cat
DriverVer = 02/18/2025,5.5.0.3366
PnpLockdown     = 1


[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MediaTek%        = MediaTek, NTAMD64.10.0...22000, NTAMD64.10.0...25336
%TPLink%          = TPLink, NTAMD64.10.0...22000, NTAMD64.10.0...25336
%MERCUSYS%        = MERCUSYS, NTAMD64.10.0...22000, NTAMD64.10.0...25336

;*******************************************************************************************
; Win11 SV3 specific entries
;*******************************************************************************************
[MediaTek.NTAMD64.10.0...25336]
; MT6639/7927
%MT6639.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_6639&SUBSYS_663914C3
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_792714C3
%MT7927.DeviceDescExA%          = MTK7927_MODE2.ndi,     PCI\VEN_14C3&DEV_7927&SUBSYS_E0E417AA
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_E0FD105B
%MT7927.DeviceDescExA%          = MTK7927_MODE3.ndi,     PCI\VEN_14C3&DEV_7927&SUBSYS_E124105B
%RZ738.DeviceDescExA%           = AMD7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_0738&SUBSYS_073814C3
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_E12F105B
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_E0FE105B
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_6639&SUBSYS_59201A3B
; MT7925
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_792514C3
%MT7925.DeviceDescExA%          = MTK7925_MODE1.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E0FF17AA
%MT7925.DeviceDescExA%          = MTK7925_MODE1.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E02517AA
%RZ717.DeviceDescExA%           = AMD7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_0717&SUBSYS_071714C3
%TO7925.DeviceDescExB%          = MTK7925_MODE7.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_8C37103C&REV_01
%TO7925.DeviceDescExB%          = MTK7925_MODE7.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_8C37103C&REV_02
%TO7925.DeviceDescExB%          = MTK7925_MODE7.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_8C38103C&REV_01
%TO7925.DeviceDescExB%          = MTK7925_MODE7.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_8C38103C&REV_02
%TO7925.DeviceDescExB%          = MTK7925_MODE7.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_8C94103C&REV_01
%MT7925.DeviceDescExA%          = MTK7925_MODE5.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_60001A3B
%MT7925.DeviceDescExA%          = MTK7925_MODE4.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_60011A3B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_60021A3B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E102105B
%AS717.DeviceDescExA%           = AMD7925_MODE2.ndi,     PCI\VEN_14C3&DEV_0717&SUBSYS_E106105B
%MT7925.DeviceDescExA%          = MTK7925_MODE4.ndi,     PCI\VEN_14C3&DEV_0717&SUBSYS_E101105B
%MT7925.DeviceDescExA%          = MTK7925_MODE5.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E10C105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E112105B
%MT7925.DeviceDescExA%          = MTK7925_MODE5.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_63701A3B
%MT7925.DeviceDescExA%          = MTK7925_MODE6.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E123105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E135105B
%RZ717.DeviceDescExA%           = AMD7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_071714C3
%MT7925.DeviceDescExA%          = MTK7925_MODE6.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E137105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E138105B
%MT7925.DeviceDescExA%          = MTK7925_MODE6.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_63731A3B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E139105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E13A105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_80051EAC
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_80061EAC
;*******************************************************************************************
;*******************************************************************************************
[TPLink.NTAMD64.10.0...25336]
; MT7927
%MT7927.DeviceDescExB%          = MTK7927_MODE1.ndi  ,   PCI\VEN_14C3&DEV_7927&SUBSYS_E104105B
; MT7925
%MT7927.DeviceDescExB%          = MTK7925_MODE2.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_60031A3B
;*******************************************************************************************

;*******************************************************************************************
[MERCUSYS.NTAMD64.10.0...25336]
%MT7925.DeviceDescExB%          = MTK7925_MODE2.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_60041A3B
;*******************************************************************************************

;*******************************************************************************************
; Win10 specific entries
;*******************************************************************************************
[MediaTek.NTAMD64.10.0...22000]
; MT6639/7927
%MT6639.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_6639&SUBSYS_663914C3
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_792714C3
%MT7927.DeviceDescExA%          = MTK7927_MODE2.ndi,     PCI\VEN_14C3&DEV_7927&SUBSYS_E0E417AA
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_E0FD105B
%MT7927.DeviceDescExA%          = MTK7927_MODE3.ndi,     PCI\VEN_14C3&DEV_7927&SUBSYS_E124105B
%RZ738.DeviceDescExA%           = AMD7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_0738&SUBSYS_073814C3
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_E12F105B
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7927&SUBSYS_E0FE105B
%MT7927.DeviceDescExA%          = MTK7927_DEFAULT.ndi,   PCI\VEN_14C3&DEV_6639&SUBSYS_59201A3B
; MT7925
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_792514C3
%MT7925.DeviceDescExA%          = MTK7925_MODE1.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E0FF17AA
%MT7925.DeviceDescExA%          = MTK7925_MODE1.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E02517AA
%RZ717.DeviceDescExA%           = AMD7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_0717&SUBSYS_071714C3
%TO7925.DeviceDescExA%          = TO7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_8C37103C&REV_01
%TO7925.DeviceDescExA%          = TO7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_8C37103C&REV_02
%TO7925.DeviceDescExA%          = TO7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_8C38103C&REV_01
%TO7925.DeviceDescExA%          = TO7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_8C38103C&REV_02
%TO7925.DeviceDescExA%          = TO7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_8C94103C&REV_01
%MT7925.DeviceDescExA%          = MTK7925_MODE5.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_60001A3B
%MT7925.DeviceDescExA%          = MTK7925_MODE4.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_60011A3B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_60021A3B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E102105B
%AS717.DeviceDescExA%           = AMD7925_MODE2.ndi,     PCI\VEN_14C3&DEV_0717&SUBSYS_E106105B
%MT7925.DeviceDescExA%          = MTK7925_MODE4.ndi,     PCI\VEN_14C3&DEV_0717&SUBSYS_E101105B
%MT7925.DeviceDescExA%          = MTK7925_MODE5.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E10C105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E112105B
%MT7925.DeviceDescExA%          = MTK7925_MODE5.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_63701A3B
%MT7925.DeviceDescExA%          = MTK7925_MODE6.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E123105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E135105B
%RZ717.DeviceDescExA%           = AMD7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_071714C3
%MT7925.DeviceDescExA%          = MTK7925_MODE6.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_E137105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E138105B
%MT7925.DeviceDescExA%          = MTK7925_MODE6.ndi,     PCI\VEN_14C3&DEV_7925&SUBSYS_63731A3B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E139105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_E13A105B
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_80051EAC
%MT7925.DeviceDescExA%          = MTK7925_DEFAULT.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_80061EAC
;*******************************************************************************************
;*******************************************************************************************
[TPLink.NTAMD64.10.0...22000]
; MT7927
%MT7927.DeviceDescExB%          = MTK7927_MODE1.ndi  ,   PCI\VEN_14C3&DEV_7927&SUBSYS_E104105B
; MT7925
%MT7927.DeviceDescExB%          = MTK7925_MODE2.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_60031A3B
;*******************************************************************************************

;*******************************************************************************************
[MERCUSYS.NTAMD64.10.0...22000]
%MT7925.DeviceDescExB%          = MTK7925_MODE2.ndi,   PCI\VEN_14C3&DEV_7925&SUBSYS_60041A3B
;*******************************************************************************************

;*******************************************************************************************
; MediaTek 7927 default configuration
;*******************************************************************************************
[MTK7927_DEFAULT.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, MldMT7927Config.reg, AFC.reg, IcmpFixRate.reg, RoamingAggreThMedLow.reg, Offload.reg, EnableSystemEventLog.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7927_DEFAULT.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7927_DEFAULT.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7927_DEFAULT.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7927 mode1 configuration
;*******************************************************************************************
[MTK7927_MODE1.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, LedCust2.reg, MldMT7927Config.reg, AFC.reg, isTPPreferBand.reg, IcmpFixRate.reg, RoamingAggreThMedLow.reg, Offload.reg, EnableSystemEventLog.reg, JPBw320Enable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7927_MODE1.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7927_MODE1.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7927_MODE1.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7927 mode2 configuration
;*******************************************************************************************
[MTK7927_MODE2.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, MldMT7927Config.reg, AFC.reg, IcmpFixRate.reg, RoamingAggreThMedLow.reg, Offload.reg, Srrc11beBiosWhiteList.reg, EnableSystemEventLog.reg, EnDropEapol.reg, EnergyStarEnable.reg, SpecialConfig.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

;*******************************************************************************************
; MediaTek 7927 Asus Mode3 configuration
;*******************************************************************************************
[MTK7927_MODE3.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, MldMT7927Config.reg, AFC.reg, IcmpFixRate.reg, RoamingAggreThMedLow.reg, Offload.reg, EnableSystemEventLog.reg, JPBw320Enable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7927_MODE3.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7927_MODE3.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7927_MODE3.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 default configuration
;*******************************************************************************************
[MTK7925_DEFAULT.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_DEFAULT.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_DEFAULT.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_DEFAULT.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 MODE1 configuration
;*******************************************************************************************
[MTK7925_MODE1.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp2.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, Srrc11beBiosWhiteList.reg, EnableSystemEventLog.reg, EnDropEapol.reg, EnergyStarEnable.reg, SpecialConfig.reg, EthernetDetectionMode2.reg, IPIFeature.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE1.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE1.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE1.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 MODE2 configuration
;*******************************************************************************************
[MTK7925_MODE2.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE2.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE2.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE2.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

[MTK7927_MODE2.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7927_MODE2.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7927_MODE2.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 MODE3 configuration
;*******************************************************************************************
[MTK7925_MODE3.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE3.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE3.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE3.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 MODE4 configuration
;*******************************************************************************************
[MTK7925_MODE4.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, Wide.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE4.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE4.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE4.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 MODE5 configuration
;*******************************************************************************************
[MTK7925_MODE5.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, Wide.reg, MldMT7925DualLinkConfig.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE5.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE5.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE5.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 MODE6 configuration
;*******************************************************************************************
[MTK7925_MODE6.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, Lso.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, DMAR.reg, EthernetDetectionMode1.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE6.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE6.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE6.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; MediaTek 7925 default MODE7 configuration (HP DMAR enable)
;*******************************************************************************************
[MTK7925_MODE7.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, Lso.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, DMAR.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[MTK7925_MODE7.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7925_MODE7.ndi.NT.HW]
AddReg                  = MSI.reg

[MTK7925_MODE7.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; HP 7925 default configuration (SV2)
;*******************************************************************************************
[TO7925_DEFAULT.ndi.NT]
AddReg                  = Common.reg, HPCurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, WiFi7Cap.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, Lso.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, DMAR.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[TO7925_DEFAULT.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[TO7925_DEFAULT.ndi.NT.HW]
AddReg                  = MSI.reg

[TO7925_DEFAULT.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; AMD 7927 configuration
;*******************************************************************************************
[AMD7927_DEFAULT.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, Dtim1.reg, FWLogToHost.reg, MldMT7927Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, DisableDynamicKAT.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[AMD7927_DEFAULT.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7927_DEFAULT.ndi.NT.HW]
AddReg                  = MSI.reg

[AMD7927_DEFAULT.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; AMD 7925 configuration
;*******************************************************************************************
[AMD7925_DEFAULT.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, DisableDynamicKAT.reg, NoStallDelayInOwnCtrl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[AMD7925_DEFAULT.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7925_DEFAULT.ndi.NT.HW]
AddReg                  = MSI.reg

[AMD7925_DEFAULT.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; AMD 7925 Mode 1 configuration
;*******************************************************************************************
[AMD7925_MODE1.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, DisableDynamicKAT.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[AMD7925_MODE1.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7925_MODE1.ndi.NT.HW]
AddReg                  = MSI.reg

[AMD7925_MODE1.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf

;*******************************************************************************************
; AMD 7925 Mode 2 configuration
;*******************************************************************************************
[AMD7925_MODE2.ndi.NT]
AddReg                  = Common.reg, CurrPhyMode.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Offload.reg, MldMT7925Config.reg, AFC.reg, RoamingAggreThMedLow.reg, EnableSystemEventLog.reg, Wide.reg, DisableDynamicKAT.reg, NoStallDelayInOwnCtrl.reg, MldMT7925DualLinkConfig.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

; New network keywords
*IfConnectorPresent     = 1   ; True
*ConnectionType         = 1   ; NET_IF_CONNECTION_DEDICATED
*DirectionType          = 0   ; NET_IF_DIRECTION_SENDRECEIVE
*AccessType             = 2   ; NET_IF_ACCESS_BROADCAST
*HardwareLoopback       = 0   ; False
NumberOfNetworkInterfaces  = 5

[AMD7925_MODE2.ndi.NT.Services]
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7925_MODE2.ndi.NT.HW]
AddReg                  = MSI.reg

[AMD7925_MODE2.ndi.NT.Wdf]
KmdfService             = %ServiceName%, wdf


;*******************************************************************************************
; Wdf version
;*******************************************************************************************
[Wdf]
KmdfLibraryVersion      = 1.33

;*******************************************************************************************
; Regs for NT
;*******************************************************************************************
[Common.reg]
HKR,,CCXPktLossLimitTime,0,"30"
HKR,,CCXDbmOffset,0,"4"
HKR,,CACDropPeriod,0,"0"
HKR,,CACDropCriteria,0,"1700"
HKR,,ConnIdleTimeForL1,0,"0"
HKR,,LowPowerEnable,0,"1"
HKR,,WirelessMode,0,"11"
HKR,,TXBurst,0,"1"
HKR,,BinMode,0,"0"
HKR,,DowngradeTxStreamFeatureEnable,0,"1"
HKR,,DowngradeTxStreamLowTempEnable,0,"1"
HKR,,DowngradeTxStreamLowTemp,0,"110"
HKR,,DowngradeTxStreamHighTempEnable,0,"1"
HKR,,DowngradeTxStreamHighTemp,0,"120"
HKR,,ShortSlot,0,"1"
HKR,,AdhocOfdm,0,"1"
HKR,,Adhoc5GDisable,0,"0"
HKR,,AdhocN40MHzAllowed,0,"0"
HKR,,WSCVersion2,0x00010001,0x00000020
HKR,,WSC20Testbed,0x00010001,0x0000000C
HKR,,MFPC,0,"1"
HKR,,InBoxMode,0,"0"
HKR,,Channel,0,%CHANNEL%
HKR,Default,Channel,0,%CHANNEL%
HKR,,RDG,0,"0"
HKR,,WMMCapable,0,"1"
HKR,,CarrierDetect,0,"0"
HKR,,MFPM3,0,"0"
HKR,,Radio,0x10001,0x7
HKR,,BatteryLifeImprove,0,"1"
HKR,,OemLedMode,0,"0"
HKR,,FwlogLevelEnable,0x00010001,"0x0"
HKR,,Country6GSPEn,0,"1"
HKLM, SYSTEM\CurrentControlSet\Services\%ServiceName%\Parameters, FWBin, 0x00010001, 1
HKLM, SYSTEM\CurrentControlSet\Services\%ServiceName%\Parameters, EnableSystemEventLog, 0x00010001, 0
HKLM, SYSTEM\CurrentControlSet\Services\%ServiceName%\Parameters, FwSramEvtBlock, 0x00010001, 1
;
; BWSelection24G
;
HKR, ,                                 BWSelection24G,          0, "0"
HKR, NDI\params\BWSelection24G,        ParamDesc,               0, %BWSelection24G%
HKR, NDI\params\BWSelection24G,        type,                    0, "enum"
HKR, NDI\params\BWSelection24G,        default,                 0, "0"
HKR, NDI\params\BWSelection24G\enum,   "0",                     0, "1. "%BW_Auto%
HKR, NDI\params\BWSelection24G\enum,   "1",                     0, "2. "%BW_20%
;
; BWSelection5G
;
HKR, ,                                 BWSelection5G,           0, "0"
HKR, NDI\params\BWSelection5G,         ParamDesc,               0, %BWSelection5G%
HKR, NDI\params\BWSelection5G,         type,                    0, "enum"
HKR, NDI\params\BWSelection5G,         default,                 0, "0"
HKR, NDI\params\BWSelection5G\enum,    "0",                     0, "1. "%BW_Auto%
HKR, NDI\params\BWSelection5G\enum,    "1",                     0, "2. "%BW_20%
;
; BWSelection6G
;
HKR, ,                                 BWSelection6G,           0, "0"
HKR, NDI\params\BWSelection6G,         ParamDesc,               0, %BWSelection6G%
HKR, NDI\params\BWSelection6G,         type,                    0, "enum"
HKR, NDI\params\BWSelection6G,         default,                 0, "0"
HKR, NDI\params\BWSelection6G\enum,    "0",                     0, "1. "%BW_Auto%
HKR, NDI\params\BWSelection6G\enum,    "1",                     0, "2. "%BW_20%
;
; BandSelection
;
HKR, ,                                 BandSelection,           0, "0"
HKR, NDI\params\BandSelection,         ParamDesc,               0, %BandSelection%
HKR, NDI\params\BandSelection,         type,                    0, "enum"
HKR, NDI\params\BandSelection,         default,                 0, "0"
HKR, NDI\params\BandSelection\enum,    "0",                     0, "1. "%Band_All%
HKR, NDI\params\BandSelection\enum,    "1",                     0, "2. "%Band24G%
HKR, NDI\params\BandSelection\enum,    "2",                     0, "3. "%Band5G%
HKR, NDI\params\BandSelection\enum,    "3",                     0, "4. "%Band6G%
;
; WakeOnMagicPacket
;
HKR, NDI\params\*WakeOnMagicPacket,             ParamDesc,      0, %WakeOnMagicPacket%
HKR, NDI\params\*WakeOnMagicPacket,             type,           0, "enum"
HKR, NDI\params\*WakeOnMagicPacket,             default,        0, "1"
HKR, NDI\params\*WakeOnMagicPacket\enum,        "0",            0, %Disable%
HKR, NDI\params\*WakeOnMagicPacket\enum,        "1",            0, %Enable%
;
; WakeOnPattern
;
HKR, NDI\params\WakeOnPattern,                 ParamDesc,      0, %WakeOnPattern%
HKR, NDI\params\WakeOnPattern,                 type,           0, "enum"
HKR, NDI\params\WakeOnPattern,                 default,        0, "1"
HKR, NDI\params\WakeOnPattern\enum,            "0",            0, %Disable%
HKR, NDI\params\WakeOnPattern\enum,            "1",            0, %Enable%
;
; ARPOffload
;
HKR, NDI\params\PMARPOffload,                  ParamDesc,      0, %ARPOffload%
HKR, NDI\params\PMARPOffload,                  type,           0, "enum"
HKR, NDI\params\PMARPOffload,                  default,        0, "1"
HKR, NDI\params\PMARPOffload\enum,             "0",            0, %Disable%
HKR, NDI\params\PMARPOffload\enum,             "1",            0, %Enable%
;
; NSOffload
;
HKR, NDI\params\PMNSOffload,                   ParamDesc,      0, %NSOffload%
HKR, NDI\params\PMNSOffload,                   type,           0, "enum"
HKR, NDI\params\PMNSOffload,                   default,        0, "1"
HKR, NDI\params\PMNSOffload\enum,              "0",            0, %Disable%
HKR, NDI\params\PMNSOffload\enum,              "1",            0, %Enable%
;
; GTKRekey
;
HKR, NDI\params\PMWiFiRekeyOffload,            ParamDesc,      0, %GTKRekey%
HKR, NDI\params\PMWiFiRekeyOffload,            type,           0, "enum"
HKR, NDI\params\PMWiFiRekeyOffload,            default,        0, "1"
HKR, NDI\params\PMWiFiRekeyOffload\enum,       "0",            0, %Disable%
HKR, NDI\params\PMWiFiRekeyOffload\enum,       "1",            0, %Enable%
;
; UAPSDSupport
;
HKR, ,                               UAPSDSupport,              0, "0"
HKR, NDI\params\UAPSDSupport,        ParamDesc,                 0, %UAPSDSupport%
HKR, NDI\params\UAPSDSupport,        type,                      0, "enum"
HKR, NDI\params\UAPSDSupport,        default,                   0, "0"
HKR, NDI\params\UAPSDSupport\enum,   "1",                       0, %Enable%
HKR, NDI\params\UAPSDSupport\enum,   "0",                       0, %Disable%
;
; AMSDUTx
;
HKR, NDI\params\AMSDUTx,        ParamDesc,               0, %AMSDUTx%
HKR, NDI\params\AMSDUTx,        type,                    0, "enum"
HKR, NDI\params\AMSDUTx,        default,                 0, "1"
HKR, NDI\params\AMSDUTx\enum,   "1",                     0, %Enable%
HKR, NDI\params\AMSDUTx\enum,   "0",                     0, %Disable%
;
; AMSDURx
;
HKR, NDI\params\AMSDURx,        ParamDesc,               0, %AMSDURx%
HKR, NDI\params\AMSDURx,        type,                    0, "enum"
HKR, NDI\params\AMSDURx,        default,                 0, "1"
HKR, NDI\params\AMSDURx\enum,   "1",                     0, %Enable%
HKR, NDI\params\AMSDURx\enum,   "0",                     0, %Disable%
;
; RSCIPv4
;
HKR, Ndi\params\*RscIPv4,        ParamDesc,               0, "RSC IPv4"
HKR, Ndi\params\*RscIPv4\enum,   "0",                     0, %Disable%
HKR, Ndi\params\*RscIPv4\enum,   "1",                     0, %Enable%
HKR, Ndi\params\*RscIPv4,        Type,                    0, "enum"
HKR, Ndi\params\*RscIPv4,        Default,                 0, "1"
HKR, Ndi\Params\*RscIPv4,        Optional,                0, "0"
;
; RSCIPv6
;
HKR, Ndi\params\*RscIPv6,        ParamDesc,               0, "RSC IPv6"
HKR, Ndi\params\*RscIPv6\enum,   "0",                     0, %Disable%
HKR, Ndi\params\*RscIPv6\enum,   "1",                     0, %Enable%
HKR, Ndi\params\*RscIPv6,        Type,                    0, "enum"
HKR, Ndi\params\*RscIPv6,        Default,                 0, "1"
HKR, Ndi\Params\*RscIPv6,        Optional,                0, "0"

HKR,,BACapability,0x10001,"0x0b834040"
HKR,Default,BACapability,0x10001,"0x0b834040"
HKR,,WifiDirectControl,0x10001,"0x84368078"
HKR,Default,WifiDirectControl,0x10001,"0x84368078"
HKR,,WfdListenChannel,0,"11"
HKR,Default,WfdListenChannel,0,"11"
HKR,,WfdPhyMode,0,"2"
HKR,Default,WfdPhyMode,0,"2"
;
; Miracast prefer band
;
HKR,,WfdGOOperatingChannel,0,"0"
HKR,NDI\params\WfdGOOperatingChannel,ParamDesc,0, "Miracast prefer band"
HKR,NDI\params\WfdGOOperatingChannel,type,     0, "enum"
HKR,NDI\params\WfdGOOperatingChannel,default,  0, "0"
HKR,NDI\params\WfdGOOperatingChannel\enum,     0,0, %WirelessModeAuto%
HKR,NDI\params\WfdGOOperatingChannel\enum,     11,0, %WirelessMode24G%
HKR,NDI\params\WfdGOOperatingChannel\enum,     36,0, %WirelessMode5G%
HKR,,P2P_GO_Band,0,"2"
HKR,Default,P2P_GO_Band,0,"2"
HKR,,Enable_U4TVBOX_FIX,0,"1"
HKR,Default,Enable_U4TVBOX_FIX,0,"1"
HKR,,P2PAckCheck,0,"1"
HKR,Default,P2PAckCheck,0,"1"
HKR,,P2PVideoBoost,0,"0"
HKR,,TransmitSetting,0x10001,"0x22d8f9"
HKR,Default,TransmitSetting,0x10001,"0x22d8f9"
HKR,,WPSDevName,0,%WPS_DEVNAME_DEF_STR%
HKR,Default,WPSDevName,0,%WPS_DEVNAME_DEF_STR%
HKR,,ProhibitTKIPonHT,0,"1"
HKR,,LinkSpeedStatus,0,"0"
;
; Low power
;
HKR, NDI\params\LowPowerEnable,        ParamDesc,               0, %LowpowerStr%
HKR, NDI\params\LowPowerEnable,        type,                    0, "enum"
HKR, NDI\params\LowPowerEnable,        default,                 0, "1"
HKR, NDI\params\LowPowerEnable\enum,   "0",                     0, %Disable%
HKR, NDI\params\LowPowerEnable\enum,   "1",                     0, %WirelessModeAuto%
;
; TxPowerLevel
;
HKR, ,                                 TxPowerLevel,0,"0"
HKR, NDI\params\TxPowerLevel,         ParamDesc,              0, %TxPowerLevel%
HKR, NDI\params\TxPowerLevel,         type,                   0, "enum"
HKR, NDI\params\TxPowerLevel,         default,                0, "0"
HKR, NDI\params\TxPowerLevel\enum,    "0",                    0, "1. "%Highest%
HKR, NDI\params\TxPowerLevel\enum,    "1",                    0, "2. "%Medium%
HKR, NDI\params\TxPowerLevel\enum,    "2",                    0, "3. "%Lowest%

[Wpp.reg]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, Start, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, BufferSize, 0x00010001, 0x50
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, ClockType, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, FileMax, 0x00010001, 0x4
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, FileName, 0, "%%SystemRoot%%\System32\LogFiles\WMI\MTK\mtkwl.etl"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, Guid, 0, "{6E7426BF-2100-4E08-9925-0F77AC45DEA6}"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, LogFileMode, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, MaxFileSize, 0x00010001, 0x32
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, MaximumBuffers, 0x00010001, 0x10
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, MinimumBuffers, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL\{04E020C0-4996-4C83-AF91-A6484F61B360}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL\{04E020C0-4996-4C83-AF91-A6484F61B360}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL\{04E020C0-4996-4C83-AF91-A6484F61B360}, EnableFlags, 0x00010001, 0x7fffffff

[Wpp2.reg]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, Start, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6A660F9B-5D03-494A-881C-26E30A3CE1B7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6A660F9B-5D03-494A-881C-26E30A3CE1B7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6A660F9B-5D03-494A-881C-26E30A3CE1B7}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6A660F9B-5D03-494A-881C-26E30A3CE1B7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E0CB17B6-C0D8-4455-9FB7-1E733AA594AF}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E0CB17B6-C0D8-4455-9FB7-1E733AA594AF}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E0CB17B6-C0D8-4455-9FB7-1E733AA594AF}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E0CB17B6-C0D8-4455-9FB7-1E733AA594AF}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{361B784D-A9F5-4659-92CD-A79774CD95A6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{361B784D-A9F5-4659-92CD-A79774CD95A6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{361B784D-A9F5-4659-92CD-A79774CD95A6}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{361B784D-A9F5-4659-92CD-A79774CD95A6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{F5751CDE-1671-496A-A738-1460C43BE40E}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{F5751CDE-1671-496A-A738-1460C43BE40E}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{F5751CDE-1671-496A-A738-1460C43BE40E}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{F5751CDE-1671-496A-A738-1460C43BE40E}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4CE7FA12-127E-4BBD-9949-C5B088742DAA}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4CE7FA12-127E-4BBD-9949-C5B088742DAA}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4CE7FA12-127E-4BBD-9949-C5B088742DAA}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4CE7FA12-127E-4BBD-9949-C5B088742DAA}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07875362-2572-4AF4-9180-1C36C818B22C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07875362-2572-4AF4-9180-1C36C818B22C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07875362-2572-4AF4-9180-1C36C818B22C}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07875362-2572-4AF4-9180-1C36C818B22C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EEDF348E-7565-4C2B-89F9-57320084B038}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EEDF348E-7565-4C2B-89F9-57320084B038}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EEDF348E-7565-4C2B-89F9-57320084B038}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EEDF348E-7565-4C2B-89F9-57320084B038}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{808460D5-F550-42F8-902D-74723FE4D9D9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{808460D5-F550-42F8-902D-74723FE4D9D9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{808460D5-F550-42F8-902D-74723FE4D9D9}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{808460D5-F550-42F8-902D-74723FE4D9D9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A94493D6-648E-4A6C-91DF-985EC049D0AE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A94493D6-648E-4A6C-91DF-985EC049D0AE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A94493D6-648E-4A6C-91DF-985EC049D0AE}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A94493D6-648E-4A6C-91DF-985EC049D0AE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{12FFFA79-16DC-4986-BDEA-6606EF03584B}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{12FFFA79-16DC-4986-BDEA-6606EF03584B}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{12FFFA79-16DC-4986-BDEA-6606EF03584B}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{12FFFA79-16DC-4986-BDEA-6606EF03584B}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07C3CBFA-D7AE-48FF-BCE2-6623346B62D4}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07C3CBFA-D7AE-48FF-BCE2-6623346B62D4}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07C3CBFA-D7AE-48FF-BCE2-6623346B62D4}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{07C3CBFA-D7AE-48FF-BCE2-6623346B62D4}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6EC664B6-A13A-4C0E-897C-1481E3AFAB17}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6EC664B6-A13A-4C0E-897C-1481E3AFAB17}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6EC664B6-A13A-4C0E-897C-1481E3AFAB17}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6EC664B6-A13A-4C0E-897C-1481E3AFAB17}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D1FF9A81-01F9-4359-A2F0-62D9F2CCED28}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D1FF9A81-01F9-4359-A2F0-62D9F2CCED28}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D1FF9A81-01F9-4359-A2F0-62D9F2CCED28}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D1FF9A81-01F9-4359-A2F0-62D9F2CCED28}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7ECDEAF5-AF6A-493B-A2D9-EC8A6A4781AE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7ECDEAF5-AF6A-493B-A2D9-EC8A6A4781AE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7ECDEAF5-AF6A-493B-A2D9-EC8A6A4781AE}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7ECDEAF5-AF6A-493B-A2D9-EC8A6A4781AE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A5AF555D-0A4E-4CCA-A649-DE861EBA1692}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A5AF555D-0A4E-4CCA-A649-DE861EBA1692}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A5AF555D-0A4E-4CCA-A649-DE861EBA1692}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A5AF555D-0A4E-4CCA-A649-DE861EBA1692}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DC8ACB45-FB1B-4F37-9B85-57708682EF51}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DC8ACB45-FB1B-4F37-9B85-57708682EF51}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DC8ACB45-FB1B-4F37-9B85-57708682EF51}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DC8ACB45-FB1B-4F37-9B85-57708682EF51}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4472937D-3D35-4BA0-AC2A-6E779B195322}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4472937D-3D35-4BA0-AC2A-6E779B195322}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4472937D-3D35-4BA0-AC2A-6E779B195322}, EnableFlags, 0x00010001, 0x7fffffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4472937D-3D35-4BA0-AC2A-6E779B195322}, Status, 0x00010001, 0x0

[FWLogToHost.reg]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, Start, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, BufferSize, 0x00010001, 0x50
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, ClockType, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, FileMax, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, FileName, 0, "%%SystemRoot%%\System32\LogFiles\WMI\MTK\mtkwlFW.etl"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, Guid, 0, "{6E7426BF-2100-4E08-9925-0F77AC45DEA6}"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, LogFileMode, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, MaxFileSize, 0x00010001, 0xc8
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, MaximumBuffers, 0x00010001, 0x10
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, MinimumBuffers, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, FWToHost, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW\{A6053918-A813-4451-9421-47845504CDAB}, Enabled, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW\{A6053918-A813-4451-9421-47845504CDAB}, EnableLevel, 0x00010001, 0x5
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW\{A6053918-A813-4451-9421-47845504CDAB}, EnableFlags, 0x00010001, 0x7fffffff

[EnableSystemEventLog.reg]
HKR,,EnableSystemEventLog,0,"1"

[DisableSystemEventLog.reg]
HKR,,EnableSystemEventLog,0,"0"

[DisableDynamicKAT.reg]
HKR,,DynamicKATEnable,0,"0"

[FWIDXLogOff.reg]
HKR,,FWIndexLogCheck,0,"0"

[IHV.reg]
HKR,Ndi\IHVExtensions, ExtensibilityDLL, 0, "%13%\mtkihvx.dll"

[IEEE80211H.reg]
HKR,,IEEE80211H,0,"0"

[WiFi7Cap.reg]
HKR,,bHideWiFi7CapOS,0,"0"

[AFC.reg]
HKR,,AFCEnable,0,"1"
HKR,,AfcBackoffPwrLimit,0,"0"

[Coex.reg]
HKR,,CoexGModeRate,0,"1"
HKR,,EnDefaultIotApRule,0,"1"

[PsControl.reg]
HKR,,PSMControl,0x00010001,0x00000000

[CountryRegion.reg]
HKR,,CountryRoamingEn,0,"1"
HKR,,SmartCountryDecisionEn,0,"0"
HKR,,DynamicCountryDecisionEn,0,"1"
HKR,,CountryRegionString,0,"WW"
HKR,,CountryDecisionNum,0,"1"
HKR,,CSSCode,0,"0"

[CountryRegion1.reg]
HKR,,CountryRoamingEn,0,"1"
HKR,,SmartCountryDecisionEn,0,"0"
HKR,,DynamicCountryDecisionEn,0,"1"
HKR,,CountryRegionString,0,"WW"
HKR,,CountryDecisionNum,0,"1"
HKR,,CSSCode,0,"F"

[LedCust1.reg]
HKR,,LedCustMode,0,"1"
HKR,,OemLedMode,0,"1"

[LedCust2.reg]
HKR,,OemLedMode,0,"2"

[isTPPreferBand.reg]
HKR,,isTPPreferBand,0,"1"

[SpecialConfig.reg]
HKR,,CrossAKMRoam,0,"0"
HKR,,OemApiSupport,0,"0"

[Wow.reg]
HKR,,WakeUpCapabilities,0x00010001,0x0005DFFF
HKR,,WakeUpFuncEnable,0x00010001,0x0007
HKR,,ETxBfNonCompressedFeedback,0,"0"

[MSI.reg]
HKR,Interrupt Management,,0x00000010
HKR,Interrupt Management\MessageSignaledInterruptProperties,,0x00000010
HKR,Interrupt Management\MessageSignaledInterruptProperties,MSISupported,0x00010001,1
HKR,Interrupt Management\MessageSignaledInterruptProperties,MessageNumberLimit,0x00010001,1

[ChannelMode.reg]
HKR,,ChannelMode,0,"1"

[IPIFeature.reg]
HKR,,EnableIPIFeature,0,"1"

[RegRemove.delReg]
HKR,,CurrPhyMode
HKR, NDI\params\CurrPhyMode
HKR,,RoamNeedIndicateTh
HKR, NDI\params\RoamNeedIndicateTh

[ThermalProtection.reg]
HKR,,ThermalEnable,0,"1"
HKR,,ThermalProtBand_A,0,"1"
HKR,,ThermalProtLV0_A,0,"100"
HKR,,ThermalProtLV1_A,0,"90"
HKR,,ThermalProtLV2_A,0,"80"
HKR,,ThermalProtLV3_A,0,"30"
HKR,,ThermalProtType_A,0,"1"
HKR,,ThermalProtTrigType_A,0,"1"
HKR,,ThermalProtTrigTemp_A,0,"115"
HKR,,ThermalProtRestoreTemp_A,0,"105"
HKR,,ThermalProtCheckTime_A,0,"5"

HKR,,ThermalProtBand_G,0,"1"
HKR,,ThermalProtLV0_G,0,"100"
HKR,,ThermalProtLV1_G,0,"90"
HKR,,ThermalProtLV2_G,0,"80"
HKR,,ThermalProtLV3_G,0,"30"
HKR,,ThermalProtType_G,0,"1"
HKR,,ThermalProtTrigType_G,0,"1"
HKR,,ThermalProtTrigTemp_G,0,"115"
HKR,,ThermalProtRestoreTemp_G,0,"105"
HKR,,ThermalProtCheckTime_G,0,"5"

[EthernetDetectionMode1.reg]
HKR,,EthernetDetection,0,"1"
HKR,,EthernetDetectionInterval,0,"2000"

[EthernetDetectionMode2.reg]
HKR,,EthernetDetection,0,"1"
HKR,,EthernetDetectionInterval,0,"5000"

[NoStallDelayInOwnCtrl.reg]
HKR,,NoStallDelayInOwnCtrl,0x00010001,0x1

[PreferBandNoPref.reg]
;
; PreferredBand
;
HKR, NDI\params\PreferredBand,        ParamDesc,       0, %PreferredBand%
HKR, NDI\params\PreferredBand,        type,            0, "enum"
HKR, NDI\params\PreferredBand,        default,         0, "0"
HKR, NDI\params\PreferredBand\enum,   "0",             0, "1. "%NoPref%
HKR, NDI\params\PreferredBand\enum,   "1",             0, "2. "%Band_24G%
HKR, NDI\params\PreferredBand\enum,   "2",             0, "3. "%Band_5G%
HKR, NDI\params\PreferredBand\enum,   "3",             0, "4. "%Band_6G%

[RoamingAggreThMedLow.reg]
;
; Roaming Aggressiveness
;
HKR, NDI\params\RoamNeedIndicateTh, ParamDesc, 0, %RoamingAggressiveness%
HKR, NDI\params\RoamNeedIndicateTh, type, 0, "enum"
HKR, NDI\params\RoamNeedIndicateTh, default, 0, "70"
HKR, NDI\params\RoamNeedIndicateTh\enum, "0", 0, "1. "%Disable%
HKR, NDI\params\RoamNeedIndicateTh\enum, "85", 0, "2. "%Lowest%
HKR, NDI\params\RoamNeedIndicateTh\enum, "80", 0, "3. "%MediumLow%
HKR, NDI\params\RoamNeedIndicateTh\enum, "75", 0, "4. "%Medium%
HKR, NDI\params\RoamNeedIndicateTh\enum, "70", 0, "5. "%MediumHigh%
HKR, NDI\params\RoamNeedIndicateTh\enum, "65", 0, "6. "%Highest%

[MldMT7925Config.reg]
HKR,,StaMloMode,0x00010001,"0x00000003"
HKR,Default,StaMloMode,0x00010001,"0x00000003"
HKR,,EnableMlsr,0x00010001,"0x00000001"
HKR,Default,EnableMlsr,0x00010001,"0x00000001"

[MldMT7925DualLinkConfig.reg]
HKR,,MloMaxLinks,0x00010001,"0x00000002"
HKR,Default,MloMaxLinks,0x00010001,"0x00000002"

[MldMT7927Config.reg]
HKR,,StaMloMode,0x00010001,"0x00000001"
HKR,Default,StaMloMode,0x00010001,"0x00000001"

[Dtim1.reg]
HKR,,DynamicDtimPeriod,0x00010001,0x8041

[Offload.reg]
HKR,,*RscIPv4,0,"1"
HKR,,*RscIPv6,0,"1"

[Lso.reg]
HKR,,*LsoV2IPv4,0,"1"
HKR,,*LsoV2IPv6,0,"1"

[Wide.reg]
HKR,,wideEn,0,"1"

[DMAR.reg]
HKLM, SYSTEM\CurrentControlSet\Services\%ServiceName%\Parameters, DMARemappingCompatible, 0x00010001, 1
HKR,,DMARsupport,0,"1"

[CurrPhyMode.reg]
;
; CurrPhyMode
;
HKR, ,                              CurrPhyMode,     0, "0"
HKR, NDI\params\CurrPhyMode,        ParamDesc,       0, %CurrPhyMode%
HKR, NDI\params\CurrPhyMode,        type,            0, "enum"
HKR, NDI\params\CurrPhyMode,        default,         0, "0"
HKR, NDI\params\CurrPhyMode\enum,   "0",             0, "1. "%Phy_11be%
HKR, NDI\params\CurrPhyMode\enum,   "1",             0, "2. "%Phy_11ax%
HKR, NDI\params\CurrPhyMode\enum,   "2",             0, "3. "%Phy_11ac%
HKR, NDI\params\CurrPhyMode\enum,   "3",             0, "4. "%Phy_11n%
HKR, NDI\params\CurrPhyMode\enum,   "4",             0, "5. "%Phy_11abg%

[HPCurrPhyMode.reg]
;
; HPCurrPhyMode
;
HKR, ,                              CurrPhyMode,     0, "0"
HKR, NDI\params\CurrPhyMode,        ParamDesc,       0, %HPCurrPhyMode%
HKR, NDI\params\CurrPhyMode,        type,            0, "enum"
HKR, NDI\params\CurrPhyMode,        default,         0, "0"
HKR, NDI\params\CurrPhyMode\enum,   "0",             0, "1. "%Phy_11ax%
HKR, NDI\params\CurrPhyMode\enum,   "1",             0, "2. "%Phy_11ac%
HKR, NDI\params\CurrPhyMode\enum,   "2",             0, "3. "%Phy_11n%
HKR, NDI\params\CurrPhyMode\enum,   "3",             0, "4. "%Phy_11abg%

[IcmpFixRate.reg]
HKR,,IcmpFixRate,0,"0"

[Srrc11beBiosWhiteList.reg]
HKR,,Srrc11beBiosWhiteList,0,"1"

[JPBw320Enable.reg]
HKR,,JPBw320Enable,0,"1"

[EnDropEapol.reg]
HKR,,EnDropEAPOL ,0,"1"

[EnergyStarEnable.reg]
HKR,,EnergyStarEnable ,0,"1"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************
[NT.CopyFiles]
mtkwecx.sys,,,2
mtkwlan.dat,,,2

[IHV.CopyFiles]
mtkihvx.dll,,,2

[SourceDisksNames]
1 = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]
mtkwecx.sys                          = 1,,
mtkihvx.dll                          = 1,,
mtkwlan.dat                          = 1,,

[DestinationDirs]
NT.CopyFiles            = 13 ; Driver Store
DefaultDestDir          = 11
CoInstaller.CopyFiles   = 11
IHV.CopyFiles           = 11 ; Windows\System32

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[MTPCI_OS61.ndi.NT.reg]
HKR,Ndi,Service,0,%ServiceName%
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet,wlan"

[Generic.Service]
DisplayName            = %Generic.Service.DispName%
ServiceType            = 1 ;%SERVICE_KERNEL_DRIVER%
StartType              = 3 ;%SERVICE_AUTO_START%
ErrorControl           = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary          = %13%\mtkwecx.sys
LoadOrderGroup         = NDIS

[common.EventLog]
AddReg      = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\netevent.dll;%%13%%\mtkwecx.sys"
HKR,,TypesSupported,0x00010001,7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio On/Off"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Preferred Band"
NoPref                      = "No Preference"
Band_24G                    = "Prefer 2.4GHz band"
Band_5G                     = "Prefer 5GHz band"
Band_6G                     = "Prefer 6GHz band"
WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Disabled"
Enable                      = "Enabled"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Roaming Aggressiveness"
Lowest                      = "Lowest"
MediumLow                   = "Medium-Low"
Medium                      = "Medium"
MediumHigh                  = "Medium-High"
Highest                     = "Highest"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Traditional Chinese 
;*******************************************************************************************
[Strings.0404]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "無線裝置 開/關"
CountryRegion24G            = "頻道代碼 (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "頻道代碼 (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒體/遊戲環境"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "偏好的頻帶"
NoPref                      = "無偏好設定"
Band_24G                    = "喜好 2.4 GHz 頻帶"
Band_5G                     = "偏好 5GHz 頻帶"
Band_6G                     = "偏好 6GHz 頻帶"
WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "禁用"
Enable                      = "啟用"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "漫遊積極度"
Lowest                      = "最低"
MediumLow                   = "中低"
Medium                      = "中"
MediumHigh                  = "中高"
Highest                     = "最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Simplified Chinese
;*******************************************************************************************
[Strings.0804]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "无线装置 开/关"
CountryRegion24G            = "频道代码 (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "频道代码(5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒体/游戏环境"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "首选频带"
NoPref                      = "无首选项"
Band_24G                    = "首选 2.4 GHz 频带"
Band_5G                     = "首选 5GHz 频带"
Band_6G                     = "首选 6GHz 频带"
WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "已禁用"
Enable                      = "已启用"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "漫游主动性"
Lowest                      = "最低"
MediumLow                   = "中低"
Medium                      = "中"
MediumHigh                  = "中高"
Highest                     = "最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "省电"
;*******************************************************************************************
; Strings --- Japanese
;*******************************************************************************************
[Strings.0411]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "無線デバイス オン/オフ"
CountryRegion24G            = "チャンネルコード  (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "チャンネルコード (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "マルチメディア/ゲーミング環境"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "優先バンド"
NoPref                      = "優先順位なし"
Band_24G                    = "2.4 GHz バンドの優先"
Band_5G                     = "5 GHz バンドを優先"
Band_6G                     = "6 GHz バンドを優先"
WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "無効"
Enable                      = "有効"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "ローミングの積極性"
Lowest                      = "最低"
MediumLow                   = "中低"
Medium                      = "中"
MediumHigh                  = "中高"
Highest                     = "最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Korean
;*******************************************************************************************
[Strings.0412]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "라디오 ON/OFF"
CountryRegion24G            = "국가/지역  (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "국가/지역 (5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "멀티미디어/게임 환경"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "기본 설정 밴드"
NoPref                      = "기본 설정 없음"
Band_24G                    = "2.4 GHz 밴드 선택"
Band_5G                     = "5GHz 밴드 기본 설정"
Band_6G                     = "6GHz 밴드 기본 설정"
WakeOnMagicPacket           = "Wake on 매직 패킷"
WakeOnPattern               = "Wake on 패턴 일치"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "비활성화함"
Enable                      = "활성화함"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "로밍의 주동성"
Lowest                      = "최하"
MediumLow                   = "보통-낮음"
Medium                      = "보통"
MediumHigh                  = "보통-높음"
Highest                     = "최고"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- French
;*******************************************************************************************
[Strings.040c]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio Marche/Arrêt"
CountryRegion24G            = "Pays / Région (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Pays / Région (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Environnements Multimédia/Jeux"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Bande privilégiée"
NoPref                      = "Aucune préférence"
Band_24G                    = "Préférer bande 2,4 GHz"
Band_5G                     = "Préférer la bande 5 GHz"
Band_6G                     = "Préférer la bande 6 GHz"
WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Correspondance au modèle WOL"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Désactivé(e)"
Enable                      = "Activé(e"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agressivité de l’itinérance"
Lowest                      = "Min."
MediumLow                   = "Faible"
Medium                      = "Moyenne"
MediumHigh                  = "Élevée"
Highest                     = "Max."

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Italian
;*******************************************************************************************
[Strings.0410]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio Acceso/Spento"
CountryRegion24G            = "Paese (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Paese (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente multimediale/giochi"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Banda preferita"
NoPref                      = "Nessuna preferenza"
Band_24G                    = "Preferenza a banda a 2,4 GHz"
Band_5G                     = "Banda a 5 GHz"
Band_6G                     = "Banda a 6 GHz"
WakeOnMagicPacket           = "Magic Packet per riattivazione"
WakeOnPattern               = "Corrispondenza motivo per riattivazione"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Disattivata"
Enable                      = "Attivata"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Efficacia roaming"
Lowest                      = "Minimo"
MediumLow                   = "Medio-basso"
Medium                      = "Medio"
MediumHigh                  = "Medio-alto"
Highest                     = "Massimo"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- German
;*******************************************************************************************
[Strings.0407]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio An/Aus"
CountryRegion24G            = "Land Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Land Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Spielumgebung"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Bevorzugtes Band"
NoPref                      = "Keine Einstellung"
Band_24G                    = "2,4-GHz-Band bevorzugen"
Band_5G                     = "5 GHz-Band bevorzugt"
Band_6G                     = "6 GHz-Band bevorzugt"
WakeOnMagicPacket           = "Aktivierung durch Magic Packet"
WakeOnPattern               = "Aktivierung durch Musterübereinstimmung"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Deaktiviert"
Enable                      = "Aktiviert"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Roaming-Dynamik"
Lowest                      = "Am niedrigsten"
MediumLow                   = "Mittel-niedrig"
Medium                      = "Mittel"
MediumHigh                  = "Mittel-hoch"
Highest                     = "Am höchsten"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Spanish
;*******************************************************************************************
[Strings.0c0a]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio Encendido/Apagado"
CountryRegion24G            = "Región País (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Región País (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente de Multimedia/Juego"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Banda preferida"
NoPref                      = "Sin preferencias"
Band_24G                    = "Preferir la banda de 2,4 GHz"
Band_5G                     = "Preferencia de banda 5 GHz"
Band_6G                     = "Preferencia de banda 6 GHz"
WakeOnMagicPacket           = "Magic Packet de reactivación"
WakeOnPattern               = "Coincidencia de patrones de reactivación"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Desactivado"
Enable                      = "Activado"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agresividad de itinerancia"
Lowest                      = "Mínimo"
MediumLow                   = "Bajo"
Medium                      = "Mediano"
MediumHigh                  = "Alto"
Highest                     = "Máximo"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Brazilian Portuguese
;*******************************************************************************************
[Strings.0416]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Rádio Ligado/Desligado"
CountryRegion24G            = "País Região (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "País Região (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente de Multimedia/Jogo"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Banda preferencial"
NoPref                      = "Sem preferência"
Band_24G                    = "Preferir banda de 2,4 GHz"
Band_5G                     = "Preferir banda de 5 GHz"
Band_6G                     = "Preferir banda de 6 GHz"
WakeOnMagicPacket           = "Pacote Mágico do Wake on"
WakeOnPattern               = "Correspondência de padrão do Wake on"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Desabilitado"
Enable                      = "Habilitado"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agressividade de roaming"
Lowest                      = "Mais baixo"
MediumLow                   = "Média a baixa"
Medium                      = "Média"
MediumHigh                  = "Média a alta"
Highest                     = "Mais alto"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Dutch
;*******************************************************************************************
[Strings.0413]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx"
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio Aan/Uit"
CountryRegion24G            = "Land regio (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Land regio (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Spelomgeving"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Voorkeursband"
NoPref                      = "Geen voorkeur"
Band_24G                    = "Voorkeur voor 2,4-GHz band"
Band_5G                     = "5 GHz band"
Band_6G                     = "6 GHz band"
WakeOnMagicPacket           = "Activeren na Magic-pakket"
WakeOnPattern               = "patroonovereenkomst"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Uitgeschakeld"
Enable                      = "Ingeschakeld"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Inc."
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agressiviteit bij roamen"
Lowest                      = "Laagste"
MediumLow                   = "Laag"
Medium                      = "Normaal"
MediumHigh                  = "Hoog"
Highest                     = "Hoogste"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
;*******************************************************************************************
; Strings --- Russian
;*******************************************************************************************
[Strings.0419]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."
TPLink                      = "TP-Link Systems Inc."
MERCUSYS                    = "MERCUSYS Technologies Co., Ltd."

MT6639.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7927 Wireless LAN Card"
MT7927.DeviceDescExB        = "TP-Link Wi-Fi 7 PCIe Adapter"
MT7925.DeviceDescExB        = "MERCUSYS Wi-Fi 7 PCIe Adapter"
RZ738.DeviceDescExA         = "RZ738 WiFi 7 320MHz"
MT7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 Wireless LAN Card"
RZ717.DeviceDescExA         = "RZ717 WiFi 7 160MHz"
TO7925.DeviceDescExA        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
TO7925.DeviceDescExB        = "MediaTek Wi-Fi 7 MT7925 160MHz PCIe Adapter"
AS717.DeviceDescExA         = "MediaTek Wi-Fi 7 MT7925(RZ717) 160MHz Wireless LAN Card"
INSTALL_DISK_STR            = "MediaTek Wireless Installation Disk"

ServiceName                 = "mtkwecx" 
Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Радио Вкл/Выкл"
CountryRegion24G            = "трана/регион (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Страна/регион (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Мультимедийная/Игровая среда"
CurrPhyMode                 = "802.11be/ax/ac/n/abg"
HPCurrPhyMode               = "802.11ax/ac/n/abg"
Phy_11be                    = "802.11be"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                    = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Предпочитаемая частота"
NoPref                      = "Нет предпочтений"
Band_24G                    = "Предпочитать частоту 2,4 ГГц"
Band_5G                     = "диапазон 5 ГГц предпочтительней."
Band_6G                     = "диапазон 6 ГГц предпочтительней."
WakeOnMagicPacket           = "Пробуждение пакетом Magic Packet"
WakeOnPattern               = "Пробуждение при соответствии шаблону"
ARPOffload                  = "ARP Offload for WOWLAN"
NSOffload                   = "NS Offload for WOWLAN"
GTKRekey                    = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Выключено"
Enable                      = "Включено"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Агрессивность роуминга"
Lowest                      = "Мин."
MediumLow                   = "Средн.-мин."
Medium                      = "Средн."
MediumHigh                  = "Средн.-макс."
Highest                     = "Макс."

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"

LowpowerStr                 = "Power Saving"
